## SPC Flooring Stone Grain

SPC Flooring’s Introduction

The main raw material of stone plastic composite flooring is natural stone powder. It does not contain any radioactive elements after being tested by the national authoritative department. It is a new green and environmental protection ground decoration material. Any qualified stone plastic composite flooring needs to pass IS09000 international quality system certification and ISO14001 international green environmental protection certification.

WhatsApp Now

### Product Detail

## SPC Flooring’s Installation Notes

1.The temperature should be kept between 10-30 °C; the humidity should be kept within 40%.
Please place SPC floors at a constant temperature for 24 hours before paving.

2. Basic ground requirements:
(1) The height difference within the 2m level shall not exceed 3mm, otherwise self-leveling cement construction is required to level the ground.
(2) If the ground is damaged, the width should not exceed 20cm and the depth should not exceed 5m, otherwise it needs to be filled.
(3) If there are protrusions on the ground, it must be smoothed with sandpaper or leveled with a ground leveler.

3. It is recommended to lay a silent pad (moisture-proof film, mulch film) with a thickness of less than 2mm first.

4. A minimum 10mm expansion joint must be reserved between the floor and the wall.

5. The maximum length of horizontal and vertical connection must be less than 10meters, otherwise it must be cut off.

6. During the installation process, do not use a hammer to forcibly hit the floor to prevent damage to the floor slot (groove).

7. It is not recommended to install and lay it in places such as bathrooms and toilets that are soaked in water for a long time.

8. It is not recommended to lay in outdoor, open-air balcony sun room and other environments.

9. It is not recommended to lay it in places that are not used or inhabited for a long time.

10. It is not recommended to lay 4mm SPC flooring in the room with area larger than 10 square meter.

### Product Parameter

PC Flooring’s size: 1220*183mm;
Thickness: 4mm, 4.2mm, 4.5mm, 5mm, 5.5mm, 6mm
Wear layer thickness: 0.3mm, 0.5mm, 0.6mm