UPVC Windows & Doors - Weathertec | Premium Energy Efficient Solutions

## SPC Flooring Wood Grain

SPC Flooring’s Introduction

The stone plastic composite flooring is only 4-6mm thick and weighs 7-8kg per square meter. In high-rise buildings, it has incomparable advantages for building load-bearing and space saving. At the same time, it has special advantages in the transformation of old buildings.

WhatsApp Now

### Product Detail

## SPC Flooring’s Advantages

The advantages of the new environmental protection stone plastic composite flooring (SPC flooring): environmental protection, E0 formaldehyde, abrasion resistance, scratch resistance, anti-skid, waterproof, anti-fouling, corrosion resistance, moth resistance, fire retardant, ultra-thin, thermal conductivity, sound-absorbing, noise reduction, lotus leaf principle, easy cleaning, impact resistance, flexibility, a variety of pavement methods, simple installation, DIY.

### SPC Flooring’s Application

The application of SPC flooring is very extensive, such as indoor families, hospitals, schools, office buildings, factories, public places, supermarkets, businesses, stadium and other places.

Education system (including schools, training centers, kindergartens, etc.)

Medical system (including hospitals, laboratories, pharmaceutical factories, nursing homes, etc.)

Commercial system (including shopping malls, supermarkets, hotels, entertainment and leisure centers, catering industry, specialty stores, etc.)

Sports system (stadiums, activity centers, etc.)

Office system (office building, conference room, etc.)

Industrial system (factory building, warehouse, etc.)

Transportation system (airport, railway station, bus station, wharf, etc.)

Home system (family indoor living room, bedroom, kitchen, balcony, study, etc.)

### Product Parameter

### SPC Flooring’s Maintenance

1. Please use a floor-specific cleaner to clean up the floor, and maintain the floor every 3-6 months.
2. To avoid scratching the floor with sharp objects, you’d better put protection pads (covers) on the table and chair feetwhen placing furniture, please don't push or pull the tables or chairs.
3. To avoid direct sunlight for a long time, you can block the direct sunlight with curtains, glass heat insulation film, etc.
4. If exposed to a lot of water, please remove the water as soon as possible, and reduce the humidity to the normal range.