UPVC Windows & Doors - Weathertec | Premium Energy Efficient Solutions

# Thermal Break Aluminum Profiles – Designed for Energy, Built for Elegance

Experience unmatched insulation, strength, and modern design — the perfect choice for sustainable architecture.

## Built for Lasting Thermal Performance

GKBM Thermal Break Profiles deliver durability, insulation, and sleek architectural appeal — built for lasting performance in every season.

### Thermal Insulation

Advanced thermal break technology that reduces heat transfer and boosts energy efficiency.

### Weather Resistance

Engineered to withstand rain, wind, and extreme climates with minimal maintenance.

### Architectural Precision

Sleek, modern profiles designed for high-performance structures with flawless alignment.

## Thermal Break Aluminum Profiles

Thermal Break Aluminum Profiles are specially engineered to reduce heat transfer between the interior and exterior environments. Designed for both residential and commercial applications, they ensure superior insulation, energy efficiency, and noise reduction while maintaining a sleek modern appearance.

- Advanced thermal barrier technology that minimizes energy loss
- Ideal for extreme weather conditions, offering excellent insulation
- Sleek, minimal design that complements contemporary architecture
- Compatible with high-performance glazing and global hardware systems
- Enhanced structural strength with long-lasting durability
- Improves indoor comfort by reducing external noise and heat

Ideal Locations: Perfect for modern homes, energy-efficient buildings, premium offices, hotels, and any space requiring thermal and acoustic insulation without compromising aesthetics.

Maximum Permissible Height: Depends on system design and glass configuration – typically supports up to 10 feet or more

Glazing Options: Single Glazing: 6mm to 10mm | Double/Triple Glazing: 20mm to 32mm

## GKBM Thermal Break Aluminum Profiles

Engineered for Energy Efficiency, Thermal Comfort, and Modern Aesthetics